Panda3D Manual: Controlling the Camera
<<prev | top | next>> |
By default, Panda3D runs a task that enables you to move the camera using the mouse. The keys to do this are: Left Button: pan left and right Right Button: move forwards and backwards Middle Button: rotate around the origin of the application Right and Middle Buttons: roll the point of view around the view axis Go ahead and try this camera control system. The problem with this camera control system is that it is sometimes awkward, it is not always easy to get the camera pointed in the direction we want. Instead, we are going to write a task that controls the camera's position explicitly. A task is nothing but a subroutine that gets called every frame. Update your code as follows:
import direct.directbase.DirectStart from direct.task import Task from direct.actor import Actor import math #Load the first environment model environ = loader.loadModel("models/environment") environ.reparentTo(render) environ.setScale(0.25,0.25,0.25) environ.setPos(-8,42,0) #Task to move the camera def SpinCameraTask(task): angledegrees = task.time * 6.0 angleradians = angledegrees * (math.pi / 180.0) base.camera.setPos(20*math.sin(angleradians),-20.0*math.cos(angleradians),3) base.camera.setHpr(angledegrees, 0, 0) return Task.cont taskMgr.add(SpinCameraTask, "SpinCameraTask") run()
The function `taskMgr.add` tells panda's task manager to call the subroutine `SpinCameraTask` every frame. This is a subroutine that we have written to control the camera. As long as the subroutine `SpinCameraTask` returns the constant `Task.cont`, the task manager will continue to call it every frame. The subroutine calculates the desired position of the camera based on how much time has elapsed. The camera rotates 6 degrees every second. The first two lines compute the desired orientation of the camera, first in degrees, then in radians. The `setPos` call actually sets the position of the camera. The `setHpr` call actually sets the orientation. The camera should no longer be underground, and furthermore, the camera should now be rotating about the clearing:
<<prev | top | next>> |