Panda3D Manual: Controlling the Camera (CXX)
<<prev | top | next>> |
Panda3D comes with a function that enables you to move the camera using the mouse. To use this, insert:
    window->setup_trackball();
just before your call to the main loop. The keys to navigate using this function are: Left Button: pan left and right Right Button: move forwards and backwards Middle Button: rotate around the origin of the application Right and Middle Buttons: roll the point of view around the view axis Go ahead and try this camera control system. The problem with this camera control system is that it is sometimes awkward, it is not always easy to get the camera pointed in the direction we want. Instead, we want to have our camera position changed every frame. Because tasks are not possible using C++, we have to write the main loop by ourselves. We can do this by making an infinite loop, in which the camera position gets updated and the function `framework.do_frame` gets called. All this function does is rendering the current frame. It returns false if the window is terminated, and the main loop should stop. Update your code as follows:
    #include "pandaFramework.h"
    #include "pandaSystem.h"

    PandaFramework framework;

    int main(int argc, char *argv[]) {
        //open a new window framework
      framework.open_framework(argc, argv);
        //set the window title to My Panda3D Window
      framework.set_window_title("My Panda3D Window");
        //open the window
      WindowFramework *window = framework.open_window();
      NodePath cam = window->get_camera_group(); //get the camera and store it
        //load the environment model
      NodePath environ = window->load_model(framework.get_models(),"models/environment");
      environ.reparent_to(window->get_render());
      environ.set_scale(0.25,0.25,0.25);
      environ.set_pos(-8,42,0);
        //do the main loop:
      Thread *current_thread = Thread::get_current_thread();
      while(framework.do_frame(current_thread)) {
        float time = clock()/100000.0; //get the time in seconds
        float angledegrees = time * 6.0; //the angle of the camera in degrees
        float angleradians = angledegrees * (3.14 / 180.0); //in radians
        cam.set_pos(20*sin(angleradians),-20.0*cos(angleradians),3); //set the position
        cam.set_hpr(angledegrees, 0, 0); //set the hpr
      }
      //close the window framework
      framework.close_framework();
      return (0);
    }
Note: It is not possible to update the camera's position while the trackball is enabled. To have this code work, you must not call the `setup_trackball()` function. The code in our home-made main loop calculates the desired position of the camera based on how much time has elapsed. The camera rotates 6 degrees every second. The first two lines compute the desired orientation of the camera, first in degrees, then in radians. The `set_pos` call actually sets the position of the camera. The `set_hpr` call actually sets the orientation. The camera should no longer be underground, and furthermore, the camera should now be rotating about the clearing:
<<prev | top | next>> |