------------------------------------------------------------------------
-- ddCopyAbs.decTest -- quiet decDouble copy and set sign to zero     --
-- Copyright (c) IBM Corporation, 1981, 2007.  All rights reserved.   --
------------------------------------------------------------------------
-- Please see the document "General Decimal Arithmetic Testcases"     --
-- at http://www2.hursley.ibm.com/decimal for the description of      --
-- these testcases.                                                   --
--                                                                    --
-- These testcases are experimental ('beta' versions), and they       --
-- may contain errors.  They are offered on an as-is basis.  In       --
-- particular, achieving the same results as the tests here is not    --
-- a guarantee that an implementation complies with any Standard      --
-- or specification.  The tests are not exhaustive.                   --
--                                                                    --
-- Please send comments, suggestions, and corrections to the author:  --
--   Mike Cowlishaw, IBM Fellow                                       --
--   IBM UK, PO Box 31, Birmingham Road, Warwick CV34 5JL, UK         --
--   mfc@uk.ibm.com                                                   --
------------------------------------------------------------------------
version: 2.57

-- All operands and results are decDoubles.
precision:   16
maxExponent: 384
minExponent: -383
extended:    1
clamp:       1
rounding:    half_even

-- Sanity check
ddcpa001 copyabs       +7.50  -> 7.50

-- Infinities
ddcpa011 copyabs  Infinity    -> Infinity
ddcpa012 copyabs  -Infinity   -> Infinity

-- NaNs, 0 payload
ddcpa021 copyabs         NaN  -> NaN
ddcpa022 copyabs        -NaN  -> NaN
ddcpa023 copyabs        sNaN  -> sNaN
ddcpa024 copyabs       -sNaN  -> sNaN

-- NaNs, non-0 payload
ddcpa031 copyabs       NaN10  -> NaN10
ddcpa032 copyabs      -NaN15  -> NaN15
ddcpa033 copyabs      sNaN15  -> sNaN15
ddcpa034 copyabs     -sNaN10  -> sNaN10
ddcpa035 copyabs       NaN7   -> NaN7
ddcpa036 copyabs      -NaN7   -> NaN7
ddcpa037 copyabs      sNaN101 -> sNaN101
ddcpa038 copyabs     -sNaN101 -> sNaN101

-- finites
ddcpa101 copyabs          7   -> 7
ddcpa102 copyabs         -7   -> 7
ddcpa103 copyabs         75   -> 75
ddcpa104 copyabs        -75   -> 75
ddcpa105 copyabs       7.10   -> 7.10
ddcpa106 copyabs      -7.10   -> 7.10
ddcpa107 copyabs       7.500  -> 7.500
ddcpa108 copyabs      -7.500  -> 7.500

-- zeros
ddcpa111 copyabs          0   -> 0
ddcpa112 copyabs         -0   -> 0
ddcpa113 copyabs       0E+6   -> 0E+6
ddcpa114 copyabs      -0E+6   -> 0E+6
ddcpa115 copyabs     0.0000   -> 0.0000
ddcpa116 copyabs    -0.0000   -> 0.0000
ddcpa117 copyabs      0E-141  -> 0E-141
ddcpa118 copyabs     -0E-141  -> 0E-141

-- full coefficients, alternating bits
ddcpa121 copyabs  2682682682682682         -> 2682682682682682
ddcpa122 copyabs  -2682682682682682        -> 2682682682682682
ddcpa123 copyabs  1341341341341341         -> 1341341341341341
ddcpa124 copyabs  -1341341341341341        -> 1341341341341341

-- Nmax, Nmin, Ntiny
ddcpa131 copyabs  9.999999999999999E+384   -> 9.999999999999999E+384
ddcpa132 copyabs  1E-383                   -> 1E-383
ddcpa133 copyabs  1.000000000000000E-383   -> 1.000000000000000E-383
ddcpa134 copyabs  1E-398                   -> 1E-398

ddcpa135 copyabs  -1E-398                  -> 1E-398
ddcpa136 copyabs  -1.000000000000000E-383  -> 1.000000000000000E-383
ddcpa137 copyabs  -1E-383                  -> 1E-383
ddcpa138 copyabs  -9.999999999999999E+384  -> 9.999999999999999E+384
